**Chapter 1**

**Introduction**

Turbulent flows in the presence of one more solid surface, referred to as wall bounded flows, are prevalent in various practical situations. Wall bounded flows are important due to their extended use in engineering applications, such as the external flow around cars, ships, and buildings, the internal flows in engine pistons, pipes and channels. Many of these flows can also include the presence of a reacting region such as the combustor of jet engine or the flame spread along walls during accidental fires. The presence of reaction zones increases the complexity of the flow as well as the difficulty to understand and predict the flows using models. Further understanding of wall bounded turbulent flows where strong velocity and temperature gradients play a major role is clearly needed. The focus of this proposal is to present the numerical frame work necessary to study the flow and heat transfer characteristics of wall bounded turbulent flows.

* 1. **Numerical approach to turbulence computation**

Often conducting wind tunnel experiments to study turbulent flows can be expensive and numerical simulations may provide an attractive low cost option. The solution of turbulent flows is possible through computational simulations that vary by their level of resolution and accuracy. The most reliable computational strategy is Direct Numerical Simulation (DNS) in which all length-scales are fully resolved; due to its unparalleled accuracy and high computational cost it is only feasible for low Reynolds number flows. At the other end of the spectrum, Reynolds Averaged Navier Stokes Equation (RANS) resolve only the mean motion and rely on modeling the entire reynolds stress tensor, it has been most widely used in the engineering community for simulation practical high Reynolds number or complex flows. However, if steady state versions of RANS equations are used it will tend to suppress large scale instabilities that are fundamental to turbulent flow transport. Large Eddy Simulations (LES) represent a compromise between DNS and RANS since it does not intend to numerically resolve all turbulent length scales, but only a fraction of the larger energy-containing scales within the inertial sub range. Modeling in then applied to represent the smaller unresolved (SGS) scales, which contain only a small fraction of the turbulent kinetic energy.


****

Figure 1. Energy Spectra for all scales of turbulent flow.

The solution of turbulent flow problems is theoretically possible through the direct numerical simulation (DNS) of the Navier Stokes equation (with appropriate boundary conditions). This method constitutes the conceptually simplest approach to the problem of turbulence. Practically, however, the cost of DNS confines this approach to simple application in terms of Reynolds number and geometry complexities. In fact, in DNS all scales of motion must be resolved, from the integral to the Kolmogorov scales. The grid size must be on the order of the largest scale. This results in a number of grid points in each direction that is proportional to the ratio between the largest and the smallest scale, L/ƞ. Defining a Reynolds number based on the integral scale L, ReL, the number of grid points will be proportional to ReL(3/4) in each direction, so a total number of points proportional to ReL(9/4) is required by DNS. Moreover, the time step of the calculation dt is limited by CFL condition, that is dt < dx/U where U is the local velocity determined by the integral time and length scale, we have that the total number of steps in time is T/dt again proportional to L/ƞ. In this way the total cost of a DNS calculation will be on the order of ReL(3). This mean that for high Re numbers, DNS takes an unrealistic time to be completed: assuming that computer power will increase by a factor of 5 every five years, Spalart [1] estimates that DNS will not be applicable for the study of the flow over an airliner or a car until 2080. In this context, large-eddy simulations (LES) presents a feasible alternative to DNS calculations since it strictly models the smallest scales of the flow. The large eddies containing the bulk of the energy, typically anisotropic and dependent on boundary conditions, are simulated directly. The fact the small, dissipative eddies are modeled helps reduce the cost of LES considerably compared to DNS.

**1.2 Classification of wall bounded flows**

Wall bounded flows are constrained by the presence of a solid wall which will enforce the no-slip condition (the velocity of the fluid at the surface must be equal to the velocity of the surface) no matter how small is the viscosity of the fluid. They may be categorized into homogenous or non-homogeneous according to certain characteristic presented along the direction of the mainstream. This feature is related to the behavior of the flow parameters after some distance or period due to a restriction imposed to the flow. Typical examples are given by flow in pipes and channels after the development section, where boundary layers collapse each other and their growing process is truncated. From this point, the flow becomes homogeneous because turbulent structures repeat cyclically and periodic conditions can be established. On the contrary, a spatially evolving boundary layer is a case of non-homogeneous flow due to the unrestricted growth downstream. The non-homogeneity showed along the flow direction makes them much more challenging to compute numerically than homogeneous flows because of the need to prescribe turbulent inflow information at the inlet of the domain at each time step.

The presence of turbulence in wall-bounded flows presents an additional challenge since they are characterized by much less universal properties than free shear flows and are thus more challenging to compute. Within the viscous sublayer, the characteristic length is set by the friction velocity and the viscosity and outside from this the distance from the wall provides the appropriate scaling. As the Reynolds number increases and the thickness of the viscous sublayer decreases, the number of grid points required to resolve the near-wall structures increases. Thus, when LES have to be applied to wall-bounded flows at moderate to high Reynolds number it is still very demanding because of the inner layer resolution. In fact, as found in Chapman [2], considering a flat plate boundary layer, the outer part has energy-carry structures on the order of the boundary layer thickness, delta. Assuming that the grid spacing is fixed in the streamwise and spanwise direction and on the order of 0.1δ, Chapman estimates a total number of grid points proportional to ReL(0.4). In the inner part of the boundary layer, on the other hand, the number of points must be based on the inner layer scales; in fact, the dimension of quasi-streamwise vortices are constant in wall units (i.e., normalized by kinematic viscosity, wall stress and fluid density). In this way, the total cost of the calculation in the inner layer is estimated to be proportional to ReL(1.8) which makes this technique only suitable for moderate Reynolds number applications.

**1.2.1 Streamwise homogeneous flows: fully developed turbulent channel**

Correct modeling of wall-bounded turbulent flows require special attention to the use of accurate boundary conditions. Furthermore, inflow turbulent conditions present additional challenges and are difficult to prescribe. In this context, fully developed turbulent channel flow can be considered from the end of the developing section, as see in figure 1.1, and do not present the shortcomings associated with the time-dependent turbulent inflow conditions and represent a valuable precise tool for analyzing the near wall turbulent structures. This can be achieved numerically by prescribing periodic boundary conditions in the homogenous directions where the computational domain is assumed to be infinite. One of the first DNS of plane channels is attributed to Kim et al [3] where in their predictions, the Reynolds number is based on the wall friction velocity and the channel half-height, Ret was 180. Years later, this investigation was followed by a number of new plane channel predictions at much higher Reynolds numbers: Moser et al [4], Leonardi [5] and Jimenez’s group [6]-[7] to name a few. More recently, Hoyas and Jimenez [8] performed direct numerical simulations on a turbulent plane channel at Ret = 2000 concluding that streamwise velocity fluctuations do not scale appropriately in wall units neither near nor away from the wall.




Figure 2. Fully Developed Planar Channel Flow Schematic.

**1.2.2 Streamwise nonhomogeneous flows: spatially-developing flows**

The case where the flow is allowed to develop naturally downstream, without any imposed restrictions, can be described as non-homogeneous in the streamwise direction. The classical canonical case of this is the spatially-developing boundary layer where if turbulent it presents a steep challenge for numerical predictions due to the specification of inflow fluctuations as a crucial boundary condition. It is observed from the literature that numerical simulations, both DNS and LES, about fully developed turbulent channel are numerous. On the contrary, numerical predictions of spatially evolving turbulent boundary layers are rather scarce because of the numerical challenge to prescribe time-dependent fluctuations at the domain inlet, which cannot be approximated by conservation equations. Therefore, simulating a streamwise evolving flow implies the selection and application of a procedure able to generate realistic turbulent inflow data with a relatively high computational cost.

Several techniques for turbulent inflow generation have been employed with different degrees of success and a comprehensive review of these methods can be found in Lund et al [9] and Moin and Mahesh [10], and more recently in Keating et al [11]. The first DNS of a spatially developing boundary layer was carried out by Spalart [12]. He used a coordinate transformation to treat the streamwise inhomogeneity of evolving boundary layers as a homogeneous flow, and, consequently, agreeable to periodic conditions. The pioneering Spalart’s approach is very ingenious but is limited to flows whose mean streamwise velocity variation is small as compared to the vertical variation, such as zero-pressure gradient (ZPG) flows. Consequently, in numerical simulations of more complex flows, both inflow and outflow boundary conditions must be established introducing an additional model for the treatment of flow leaving the domain. Originally, inflow conditions were generated by specifying a mean velocity profile and superimposing some random fluctuations, so called synthetic turbulence. Le and Moin [13] and produced inflow conditions for DNS of a backward-facing step basically from a three dimensional, divergence free field of random fluctuations with prescribed moments and spectra. Random fluctuations were created by the proposed method of Lee et al [14]. Thus, this turbulent field was convected through the inflow plane by using the Taylor’s hypothesis. However, the inlet turbulent structures required a long distance for accommodation and reaching a realistic state because the inflow information was void of the phase information of the real turbulent eddies. It was reported by Le and Moin [13] that 50 displacement thicknesses from the inlet channel were required to get a realistic turbulent flow, which seriously penalized the streamwise length of the computational box and, thus, increased the cost of the simulation. An improvement of the previous approach was proposed and tested by Na and Moin [15], and Akselvoll and Moin [16] by convecting an instantaneous turbulent field computed from an auxiliary temporal simulation. This modification was observed to shorten significantly the evolution distances but at a high computational cost of having an extra numerical simulation.

More recently, Batten et al [17] introduced a new method to generate synthetic turbulence that takes into account the anisotropy of the flow. The method by Batten et al is based on the superposition of sinusoidal modes with random frequencies and wave-numbers, with given moments and spectra. Their approach includes an ingenious way to modify the wave numbers to yield eddies that are more elongate in the direction of larger Reynolds stresses, thus introducing more realistic anisotropic eddies into the flow. Spille-Kohoff [17] recently proposed a method that seeks to establish the correct Reynolds stress profiles earlier in the domain. They used a synthetic turbulent field at the inflow and a number of control planes downstream. At these planes, a controller amplifies the wall-normal velocity fluctuations to try to match the required Reynolds shear stress. This last two methods are further analyzed in turbulence validation section of chapter 4. Finally, the simulations of even more complex evolving flows, of great need in engineering applications, require the use of appropriate methodologies for inflow conditions which is part of the focus of the present study.




Figure 3. Canonical boundary layer flow schematic.

**1.3 Transport of scalars in wall-bounded flows**

The transport of scalars is important in various engineering applications ranging from combustors, boilers to thermal boundary layers as found in turbine blade film cooling. In many cases, there is a two way coupling between the scalars and the flow: the transported field can influence the velocity field – which is known as active scalar transport. This is the case, for example, of the temperature field that acts on velocity through buoyancy forces. Conversely, situations where the feedback of the scalar field is negligible and the velocity determines the properties of the scalar, but not vice versa, are termed passive. This ideal case is well approximated by the use of dye in laboratory experiments or by the transport of smoke and low concentration pollutants. Although active and passive scalars are governed by the same advection-diffusion equation, their nature is radically different. Passive scalars belong to the category of linear problems, despite being highly nontrivial. Celani et al [18] reports that as a consequence of the statistical independence of the temperature fields and the advecting velocity, the transported field depends linearly on the temperature. This property allows a theoretical treatment of the problem, and has the major consequence that the passive scalar scaling laws are universal with respect to the injection mechanism. On the contrary, for active fields, the presence of the feedback couples the velocity with the transported scalar and makes the problem fully nonlinear. In this case, the theoretical tools developed for studying the passive problem may fall short of explaining the behavior of active scalars, and the current understanding of active turbulent transport lags far behind the knowledge accumulated on the passive counterpart.

One of the first numerical simulations with respect to the transport of passive scalar fields was performed by Kim and Moin [19] at a Reynolds number of 180 (based on wall friction velocity and channel-half width) and at various molecular Prandtl numbers. They considered two different types of boundary conditions. In the first case, the scalar is generated internally and removed from isothermal walls at the same temperature. In the second case, the isothermal boundary condition is applied with walls at different temperatures, which means that the scalar is introduced at one wall and removed from the other. More recent work of DNS of turbulent heat transfer in channels have been performed and a comprehensive progress of the topic can be found in Kasagi and Iida [20], Kasagi et al [21] and Keating [11].

In the following sections, a literature review of investigations on active scalars is presented for streamwise homogeneous and non-homogeneous wall bounded flows.

* + 1. **Fully developed turbulent channel with heat transfer**

The case of streamwise homogenous flows with strong heat transfer and variable property

has been studied extensively by various researchers. Two regimes of interest often found in the literature with this configuration are: subsonic, low Mach number flow and compressible high Mach number flow; where the role of pressure becomes vital in understanding the difference between the two methods. Fully compressible numerical formulations are constrained by the need to resolve fast acoustic wave motions; hence the density is dependent on both temperature and pressure increasing the complexity of the system. In the low Mach number limit where density becomes nearly constant, the role of pressure is to act on velocity through continuity so that conservation of mass is satisfied. For low speed flows, the pressure gradient needed to drive the velocities through momentum conservation is of such magnitude that the density is not affected significantly and the flow can be considered nearly incompressible. Hence, density and pressure are very weakly related. Thus for slow flows, the low Mach number formulation, where the acoustic properties are filtered out becomes a computationally cost efficient method to use.

One of the first variable property channel flow numerical study was carried out by Wang and Pletcher [23]. They performed an LES study of low Mach number isothermal channel flows with one hot wall and one cold wall, with temperature ratios as high as3. The hot wall corresponded to heating, and the cold wall corresponded to cooling. The heat transferred to the hot wall was removed from the channel through the cold wall so there was no bulk temperature rise. Results showed the minimum velocity fluctuations at the center because there was no mean velocity gradient at that location. However, the temperature fluctuations remained large near the center of the channel. Since there is energy transfer from the heated to the cooled wall, the whole domain contains temperature gradients including the center of the channel. The compressible formulation of the dynamic SGS model was utilized in a staggered grid finite volume method that was fully implicit.

Nicoud and Poinsot [24] applied DNS to a very similar configuration and pointed out that some of the observed effects might be explained through the different local values of Reynolds number obtained near the hot and cold walls. The higher Reynolds number was observed near cold wall and lower one was found near the hot wall. The variations in Reynolds number were thought to be responsible for a variation in the size of the turbulent structures. The structures near the hot wall were much larger than values near the cold wall. These different Reynolds numbers were obviously due to different density and viscosity values which were functions of temperature. This configuration will be explained in more detail in the LES validation chapter of this proposal.

* + 1. **Natural convection heat transfer**

Modeling transport in thermal boundary layers is the main objective of this proposal. The target configuration corresponds to a non-homogeneous natural convecting shear layer obtained through the interaction of a hot surface in quiescent surrounding fluid. This configuration has been extensively studied analytically, experimentally and more recently computationally. A similarity solution was carried out by Ostrach [25] for various Prandtl numbers which were in good agreement with previous experiments and is now a classical problem for flows in the laminar regime.

Turbulent natural convection boundary layer next to a heated vertical surface was analyzed by George & Capp [26] by classical scaling arguments. In this theoretical investigation, the boundary layer is treated in two parts. An inner region in which the mean convection terms are negligible and is identified as a constant heat flux layer and an outer region which constructs most of the boundary layer in which conduction terms are considered negligible. In this work, universal velocity and temperature profiles for asymptotic values of Rayleigh number (approaching infinity) are suggested for both constant heat flux and constant temperature boundary conditions. The proposed theory was modified later by Wosnik & George [27] and it was claimed that the new scaling functions were valid both in the limit of infinite Rayleigh number and for any position downstream well into the turbulent regime. It was also shown that the boundary layer showed no linear expansion for moderate Rayleigh numbers but asymptotically lost its stream-wise inhomogeneity where it expanded linearly.

Turbulent transport in a natural convection along a vertical at plate was been studied experimentally and it was shown that the large eddy motions play an important role on the turbulent transport. Tsuji & Nagano [28] performed an experimental study of natural convecting heat transfer boundary layer in detail compared to previous researches. Characteristics of the near wall region was studied and applicability of the conventional analogy between heat and momentum transfer and the concept of the viscous sublayer for natural convection were investigated. The structure of turbulent natural convection boundary layer was studied further by Tsuji & Nagano [29] and it was shown that this phenomenon has a unique turbulent structure which is rarely seen in other turbulent boundary layers.

Natural convecting boundary layer has also been studied numerically. Many investigations have been carried out and useful results are proposed. Considering RANS computations, a v2-*f* and a k-ε model were compared with the experimental data for two different geometries by Tiezen et al [30] while at CTR Stanford University. The two considered geometries were a vertical plate and a differentially heated cavity. Three treatments of buoyancy/turbulence coupling were compared and it was shown that v2-*f*, model together with employment of a buoyant production term which was defined based on generalized diffusion hypothesis yielded the best results.

Peng & Davidson [31] studied the LES of turbulent flow in a confined cavity and compared the results with the experiment of Tian & Karayiannis [32] and Tian & Karayiannis [33]. It was shown that mean flow quantities were in good agreement with the experimental results, however, there were some discrepancies in the prediction of turbulence statistics especially in the shear layer region between the wall boundary layer flow and the cavity core region. It is suggested that special attention should be paid to the flow physics and numerical treatment in this region. A comparative study of LES of turbulent buoyant flow in a cavity with different SGS models and grid resolutions was also performed by Peng & Davidson [34]. It was shown that although the proposed SGS model was able to predict mean flow quantities, it was unable to recreate the turbulence quantities particularly in the core region. It was also shown that the energetic flow structures which are enhanced by buoyancy in the boundary layer along the heated and cooled walls of the cavity, exist in the outer layer neighboring the nearly stagnant core region of the cavity. Using DNS, Natural convection between two vertical differentially heated walls was studied by Nieuwstadt & Versteegh [35]. The major topic of investigation in this study was the self-similarity behavior of the results following the scaling hypothesis proposed by George & Capp [26]. It was shown that the proposed scaling approach leads to self-similarity for the mean temperature profile but it fails for the mean velocity profile. In another study, Versteegh & Nieuwstadt 36] investigated the turbulent budgets of natural convection in an infinite, differentially heated, vertical channel. It was found that close to the wall, the shear production of turbulence was negative. It was also mentioned that modeling of pressure strain and transport terms in a separated way is not a good idea while the combination of these two terms behaves in a more continuous way especially near wall.

* 1. **Outline of current work**

The main objective of this dissertation is to present the development of an in-house low-mach number boundary layer solved with LES capabilities. The main feature of this new software is its ability to handle variable density flows while using advanced turbulence models. It is intended to be a prediction tool that can provide high-fidelity, high resolution numerical studies of laboratory experimental configurations. This proposal organized as follows: The numerical methods and LES variable density developments are discussed and presented in Chapter 2. Chapter 3 presents validation studies of forced convection boundary layers and classical results from laminar and turbulent flows with and without heat transfer. Chapter 4 presents another validation study conducted in the natural convection regime, results from the classical Ostrach solution is presented as well as the classical result from Tsuji & Nagao and the fidelity of the code is established. Lastly, Chapter 5 presents the direction and outline of future work, including further development and validation plans to address turbulent boundary layer combustion problems.

**References**

[1] Spalart, P.R., “Strategies for turbulence modeling and simulations”, Int. J. Heat and Fluid Flow (2000), 21, 252-263.

[2] Chapman, D.R., “Computational aerodynamics, development and outlook”. AIAA J 17 1293-1313.

[3] Kim, J., Moin, P., Moser, R., "Turbulence statistics in fully developed channel flow at low Reynolds number**",** J**.** Fluid Mech(1987),177**,** 133-166**.**

[4] Moser, R., Kim, J., Mansour, N., “Direct Numerical Simulation of turbulent channel flow up to Re = 590”, Physics of Fluids (1999), vol 11, 4, 943-945.

[5] Leonardi, S., “Turbulent channel flow with roughness: direct numerical simulations”, PhD Thesis (2002), University of Rome, La Sapienza.

[6] Jimenez J, Moin P., The minimal flow unit in near-wall turbulence. *J. Fluid Mech (1991) .*225:213–40

[7] Jimenez, J., Hoyas, S., "Turbulent fluctuations above the buffer layer of wall-bounded flows", J. Fluid Mech.Vol (2008). 611. 215-236.

[8] Hoyas, S., Jimenez, J., “Scaling of velocity fluctuations in turbulent channels up to Ret = 2000”, Physics of Fluids (2006), vol 18, 011702.

[9] Lund, T.S., Moin, P., “Large eddy simulation of concave wall boundary layer”, Int. J. Heat and Fluid Flow (1996), vol 17, 290-295.

[10] Moin, P., Mahesh, K., “Direct Numerical Simulations: A tool in turbulence research”, Ann. Rev. Fluid. Mechanics (1998), vol 30, 539-578.

[11] Keating, A., “Large eddy simulation of heat transfer in turbulent channel flow and in the turbulent flow downstream of a backward facing step”, PhD Thesis (2003), University of Queensland.

[12] Spalart, P.R., “Direct simulation of a turbulent boundary layer up to Reθ = 1410”, (1988), J. Fluid Mech. 187, 61–98.

[13] Le, H., Moin, P., Kim, J., “Direct numerical simuations of turbulent flow over a backward facing step” Journal of Fluid Mechanics (1997), vol 330, 349-374.

[14] Lee S, Lele SK, Moin P., “Simulation of spatially evolving compressible turbulence and the applicability of Taylor’s hypothesis”. Physics of Fluids (1992)*,* vol4, 1521–30.

[15] Y, Na., Moin, P., “Direct numerical simulation of turbulent boundary layers with adverse pressure gradient and separation”, Tech Report TF-68 (1996), Themoscience Division, Department of Mechanical Engineering, Stanford University.

[16] Akselvoll, K. & Moin, P**.** “Large-eddy simulation of turbulent confined coannular jets”, Journal of Fluid Mech (1996), vol 315, 387-411.

[17] P. Batten, U. Goldberg, and S. Chakravarthy, Interfacing statistical turbulence closures with large-eddy simulation, AIAA J (2004, vol 42(3):485–492.

[18] A. Celani, M. Cencini, A. Mazzino, M. Vergassola , “Active and passive fields face to face” New J. Phys (2004). vol 6, 1-35.

[19] Kim, J., Moin, P., “Transport of passive scalars in a turbulent channel flow”, Turbulent Shear Flows (1989), vol 6, Springer, Berlin.

[20] Kasagi, N., Iida, O., ‘‘Progress in Direct Numerical Simulation of Turbulent Heat Transfer,’’ Proceedings of the 5th ASME/JSME Joint Thermal Engineering Conference (1999), San Diego, CA.

[21] Kasagi, N., Tomita, Y., Kuroda, A., “Direct numerical simulation of passive scalar field in a turbulent channel flow”, Journal of Heat Transfer (1992), vol 114, 598-606.

[22] Kawamura, H., Abe, H., Matsuo, Y., “Direct numerical simulation of turbulent heat transfer in channel flow with respect to Reynolds and Prandtl number effects”, Int. Journal of Heat and Fluid Flow (1999), vol 20, 196-207.

[23] Wang, W., Plechter, R., “On the large eddy simulation of a turbulent channel flow with significant heat transfer”, Physics of Fluids, vol 8, No 12, pp3354- 3366.

[24] Nicoud, F., Poinsot, T., “Direct numerical simulation of a channel flow with variable properties”, First International Symposium on Turbulence and Shear Flow Phenomena (1999), S. Banerjee and J. Eaton Editors, Santa Barbara, USA.

[25] Ostrach, S. “An analysis of laminar free-convection flow and heat transfer about a plate parallel to the direction of the generating body force”. Report 1111 (1999). NACA.

[26] George, W. K., Capp, S. P., “A theory for natural convection turbulent boundary layers next to heated vertical surfaces”. International Journal of Heat and Mass Transfer (1979), vol **22**, 813-826.

[27] Wosnik, M. & George, W. K., “Another look at the turbulent natural convection boundary layer next to heated vertical surfaces”. In ICHMT Symposium on Turbulence, Heat and Mass Transfer (1995). Lisbon.

[28] Tsuji, T. & Nagano, Y., “Characteristics of a turbulent natural convection boundary layer along a vertical flat plate”. International Journal of Heat and Mass Transfer (1988a), vol 31, 1723-1734.

[29] Tsuji, T. & Nagano, Y., “Turbulence measurements in a natural convection boundary layer along a vertical fat plate”. International Journal of Heat and Mass Transfer (1988b), vol31(10), 2101-2111.

[30] Tieszen, S., Ooi, A., Durbin, P. & Behnia, M., “Modeling of natural convection heat transfer”. Proceedings of the summer program: Center for turbulence research (1998), 287-302.

[31] Peng, S., Davidson, L., *“*Comparative study of LES for turbulent buoyant flow in terms of SGS model and grid resolution”. In The Second International Symp. on Turbulence and Shear Flow (2001), vol. 2, pp. 455.460. Stockholm.

[32] Tian, Y.S., Karayiannis, T.G., “Low turbulence natural convection in an air filled cavity part I: the thermal and fluid flow fields”, Int. Journal of Heat and Mass Transfer (2000a), vol 43, 849-866.

[33] Tian, Y.S., Karayiannis, T.G., “Low turbulence natural convection in an air filled cavity part II: the turbulence quantities”, Int. Journal of Heat and Mass Transfer (2000b), vol 43, 867-884.

[34] Peng, S., Davidson, L, “Large eddy simulation for turbulent buoyant flow in a confined cavity”, International Journal of Heat and Fluid Flow (2001), vol 22, 323-331.

[35] Nieuwstadt, F., Versteegh, T., “Direct numerical simulation of natural convection between two vertically differentially heated walls”, In Proc 11th Symp on Turbulent Shear Flows (1997), Grenoble.

[36] Versteegh, T., Nieuwstadt, F., “Turbulent Budgets of natural convection in an infinite differentially heated vertical channel”, Int. Journal of Heat and Fluid Flow (1998), vol 19, 135-149.